For 1990-2009 cars

# INT./EXT. PAINT CODES- MOLDINGS AND STRIPING COLORS

The listings of 1983 paint codes contained in this bulletin will help enable dealers to order the necessary paint materials required for effective pre-delivery preparation.

The list of colors indicates the suppliers' ordering codes for exterior, interior, vinyl roof molding, and paint stripe colors. The list also identifies those materials that are carryover in each group from the 1982 materials.

The listed paint suppliers have indicated that there are stocks of 1983 model colors in each of their field warehouses or regional distributorships.

Other manufacturers produce service paint which could perform satisfactorily for field repairs. Paint suppliers in your area can provide you with information regarding these materials.

1983 CADILLAC EXTERIOR COLORS

Sherwin- GM Paint Williams Martin Code Color Name R-M(Inmont) Ditzler DuPont Acme/Rogers Senour ---- ---------- ----------- ------- ------ ----------- ------ 11* Cotillion White 2080 2058 5338 5644 30-3929 15 Silver Sand 13100 3520 C8301 33188 30-5256 19* Sable Black A946/P403 9300 99 3000/4590 3069 22 Balboa Blue 13106 3522 B8308 32895 30-5229 27 Hatteras Blue 13110 3525 B8304 32701 30-5179 42 Grayfern 13114 3526 B8309 32902 30-5234 48 Loden Green 13115 3528 B8303 32702 30-5180 50 Cameo Ivory 13116 3529 B8318 32703 30-5181 60 Sand Gray 13120 3530 B8307 32704 30-5182 62 Woodland Haze 13121 3531 B8310 32896 30-5230 64 Antique Saddle 13125 3533 B8319 33238 30-5257 67 Briar Brown 13127 3534 B8305 32705 30-5183 74 Autumn Maple 13131V 3532 B8385 33074 30-5244 78 Royal Maroon 13132F 3553 C8310 33075 30-5245 81 Garnet 13142V 3544 C8305 33239 30-5258 82 Midnight Sand Gray 13134 3537 B8399 33076 30-5246 90 Midnight Blue 13136 3539 B8313 32986 30-5240 91 Flaxen 13137 3540 C8303 33240 30-5259 92 Briar 13138 3541 B8315 32708 30-5186 93 Sonora Saddle 13139D 3542 C8304 33241 30-5260 94 Beech 13140 3543 B8317 32710 30-5188

*Carryover 1982 colors

Underlined numbers indicate original equipment paint used in Detroit production. Linden production supplier is Inmont (except for Code 91 which is supplied by R-M).

1983 CADILLAC INTERIOR COLORS

Sherwin- Williams Acme/ Martin Trim Code Color Name R-M No. Ditzler DuPont Rogers Senour ---------- ---------- -------- ------- ------ ------ ------ 112,113,114 White 4402 (Semi) 8855* 9625* 90682* 32-16056* (UCV) 2-183* 192,193,194 Black 4401* (Semi) 9387* 4428* 90681* 32-16082* Black 12812* (Flat) 9433* 92387* 32-16615* (UCV) 120* 22B,22C,22D,22G, 22H,222,223,224 Med Dk Royal 13191D (Semi) 15680 C8385 32839 32-17018 Blue Med Dk Royal 13253D (Flat) 32936 32-16875 Blue

(UCV) 2-1033 42B,42D,422,424 Med Grayfern 13187D (Semi) 33586 C8386 32840 32-17019 Med Grayfern 13256D (Flat) 33619 32852 32-17024 Dk Grayfern 13186 (Semi) 33587 C8327 32836 32-17015 Dk Grayfern 13250 (Flat) 33620 32935 32-16874 502,504 Lt Yellow 9558* (Semi) 82379* 45227* 92346 32-16601 Lt Yellov 11528 (Flat) 32351 36-16992 Dk Yellow 9559* (Semi) 82380* 45228* 92345 32-16602 Dk Yellow 12815 (Flat) 82381* Very Dk Yellow 13185 (Semi) C8344 Very Dk Yellow 12816* (Flat) 82446* (UCV) 2-723 Med Waxberry (Semi) 82473 31199 32-1677-5 (Flat) (UCV) 2-781 Med Dk Waxberry (Semi) 82478 31327 32-16786 (Flat) 82480 (UCV) 2-807 58B,58C,58D,58G, 58H,582,583,584 Med Beech 13184 (Semi) 25194 C8332 32892 32-17025 Med Beech 13254 (Flat) 25263 32937 32-16876 Dk Beech 13183 (Semi) 25227 C8333 32976 32-16902 Dk Beech 13255 (Flat) 25264 32938 32-16877 602,603,604 Lt Sand Gray 13182 (Semi) 33567 C8384 32837 32-17016 Lt Sand Gray 13151 (Flat) 33617 32850 32-17022 Charcoal 13194 (Semi) 33568 Charcoal 13257 (Flat) 33618 (UCV) 2-973 67B,67C,67D,67G, 67H,672,673,674 Dk Briar 13175D (Semi) 25306 C8383 32835 32-17014 Dk Briar 13249D (Flat) 32934 32-16873 (UCV) 2-1043 742,743,744 Dk Carmine 9567 (Semi) 72273* 45224*92348 32-16598 Dk Carmine 13258 (Flat) 72291* (UCV) 2-570* 77B,77C,77D,77G, 77H,772,773,774 Dk Maple 12271F (Semi) 72415 C8115 31201 32-1677 Dk Maple 13258F (Flat) 72435 31423 32-16803 (UCV) 2-803

* Denotes carryover 1982 color

1983 CADILLAC VINYL ROOF MOLDING COLORS

Sherwin- Paint R-M Ditzler Williams Martin Code Color Name (Inmont) (UCV) DuPont Acme/Rogers Senour ---- ---------- --------- ----- ------ ----------- ------ 11 White 4415 183 D8369 11510 32-26885 15 Silver Sand 13157 2-952 D8370 33173 32-26636 19 Black 4416* 120* D8368 9739* 32-16082* 22 Lt Royal Blue 13158 2-953 D8382 33185 32-26648 27 Med Dk Royal Blue 13159D 2-954 D8372 33175 32-26638 42 Lt Grayfern 13160 2-955 D8383 33186 32-26649 48 Dk Grayfern 13161 2-956 D8371 33174 32-26637 50 Flax 13162 2-957 D8377 33180 32-26643 62 Lt Briar Brown 13164 2-959 D8384 33187 32-26650 67 Dk Briar Brown 13165 2-960 D8373 33176 32-26639 74 Autumn Maple 12786M 2-895 D8386 32415 32-26560 78 Dk Autumn Maple 13166D 2-961 D8374 33177 32-26640 90 Dk Royal Blue 13167G 2-962 D8376 33179 32-26642 91 Lt Flax 13168 2-966 D8378 33181 32-26644 92 Med Briar Brown 13169 2-963 D8379 33182 32-26645 93 Lt Beech 13170 2-964 D8380 33183 32-26646 94 Dk Beech 13171 2-965 D8381 33184 32-26647

1983 CADILLAC PAINT STRIPE COLORS

Sherwin- Sales R-M William Martin Code Color Name (Inmont) Ditzler DuPont Acme/Rogers Senour ---- ----------- -------- ------- ------ ------------ ------ 11A White 2080 0847* 5338 5644 32-3929 15A Sand Gray 13120 3530 B8307 33164 32-26627 19A Black A946* 9300* 99* 300/4590* 3069* 22A Lt Royal Blue 13281 15674 C8392 33153 32-26616 27A Med Dk Royal Blue 13282D 15639 C8393 33154 32-26617 42A Lt Grayfern 13283 32018 C8398 33158 32-26621 48A Dk Grayfern 13284 33006 C8399 33159 32-26622 51A Dk Flax 13262 24687 C8397 33157 32-26620 62A Lt Briar Brown 13285 25217 C8389 33151 32-26614 66A Orange 9500D* 60909* 45261* 25455* 32-26337* 67A Dk Briar Brown 13274 24945 D8328 33165 32-26628 75A Red 4518R 72128 43592 11892 32-26272 78A Dark Maple 13275R 51127 D8329 33166 32-26629 93A Lt Beech 13260 25219 D8394 33155 32-26618 94A Dk Beech 13261 25220 D8395 33156 32-26619

*Denotes carryover 1982 color

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.