For 1990-2009 cars

# LABOR TIME GUIDE (LTG) REV.S

#### SUBJECT: 1991 LABOR TIME GUIDE (LTG) REVISIONS

Time allowances for Computer Command Ride (CCR), Remote Keyless Entry (RKE), and 4T60E transaxle were omitted from the 1991 LTG initial printing. These time allowances are being published in this bulletin so you will have them prior to the 1991 LTG first revision in December. If you have any questions or comments, please call Jeff Clark on (313) 554-6946 or submit a Request For Review.

DESCRIPTION LABOR OP C D E K V --------------------------------------------- -------- ------------------ Computer Command Ride (CCR) Components - Replace Controller/Module N5600 .5 - .2 .2 .2 Lateral Accelerator Switch N5610 .4 - .7 .7 - Telltale Bulb N5620 .2 - - - - --------------------------------------------- -------- ------------------ Receiver, Remote Door/Rear Compartment Lock - Replace R4480 .8 - .2 .2 -

Battery, Remote Door/Rear Compartment Lock Transmitter - Replace R4485 .2 - .2 .2 -

Transmitter, Remote Door/Rear Compartment Lock - Replace R4490 .2 - .2 .2 - --------------------------------------------- -------- ------------------ Transaxle Oil Leak - Analyze K6105 .5 - .5 .5 -

Indicator, Transmission Oil Level (Dipstick) - Replace K6130 .2 - .2 .2 -

Tube and/or Seal, Transaxle Filler - Replace K6140 .4 - .4 .4 -

Modulator and/or Seal - Replace K6180 .4 - .4 .4 -

Bolts,Torque Converter to Flywheel - Replace K6300 .6 - .6 .6 -

Sensor, Transaxle Speed - Replace K6310 .3 .4 .6 6 .3

Housing and/or Housing-to-Case O-Ring Seal or Gasket Extension - Replace K6390 1.5 - 1.5 1.5 - --------------------------------------------- -------- ------------------ Carrier and Differential Final Drive Assembly, Final Drive Sun Gear, Parking Gear, and Final Drive Sun Gear Shaft - R&R or Replace

Carrier and Differential Final Drive Assmb. K6395 1.7 - 1.7 1.7 - Final Drive Sun Gear K6396 1.7 - 1.7 1.7 - Parking Gear K6397 1.7 - 1.7 1.7 - Final Drive Sun Gear Shaft K6398 1.7 - 1.7 1.7 - --------------------------------------------- -------- ------------------ Pan and/or Gasket, Transaxle Oil - Replace K6500 .6 - .6 .6 -

Accumulator Assembly 1-2, 2-3, - R&R or Replace K6507 .8 - .8 .8 -

Servo Assembly, Manual 2-1 - R&R or Replace K6508 .8 - .8 .8 -

Cover and/or Gasket, Valve Body - Replace K6540 2.4 - 2.1 2.1 - --------------------------------------------- -------- ------------------ Wiring Harness - Replace Harness Assembly K6554 2.6 - 2.6 2.6 -

A Solenoid K6555 2.6 - 2.6 2.6 -

B Solenoid K6556 2.6 - 2.6 2.6 -

PWM Solenoid K6557 2.6 - 2.6 2.6 -

TCC Solenoid K6558 2.6 - 2.6 2.6 - --------------------------------------------- -------- ------------------ Valve Body and Oil Pump Assembly - R&R or Replace K6570 3.4 - 3.4 3.4 - ADD: A - To Clean and Recondition Valve Body 1.0 - 1.0 1.0 - B - To Recondition Oil Pump .4 - .4 .4 - C - To Oil Pressure Test .5 - .5 .5 - --------------------------------------------- -------- ------------------ Servo Assembly, Reverse - R&R or Replace K6623 1.9 - 1.9 1.9 - ADD: To Recondition Servo .2 - .2 .2 -

Servo Assembly, Forward - R&R or Replace K6624 .5 - .5 .5 - --------------------------------------------- -------- ------------------ Mount and/or Bracket, Transaxle - Replace Right K6720 - - .2 .2 - Left K6721 - - .9 .9 - Front K6722 .5 - - - - Rear K6723 - - .5 - - Right .7 - - - - Left .7 - - - - --------------------------------------------- -------- ------------------ Seal, Transaxle Axle Shaft Oil - Replace Right K6900 .8 - .8 .8 - Left K6900 .8 - .8 .8 - Both K6907 1.4 - 1.4 1.4 - --------------------------------------------- -------- ------------------ Shaft, Transaxle Output - Replace K6940 6.5 - 6.5 6.5 - --------------------------------------------- -------- ------------------

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.