For 1990-2009 cars

# SMU - SECTION 9J-A-29 REVISION TO CHART G IN SIR

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 9J-A-29 - REVISION TO CHART G - DERM CANNOT COMMUNICATE WITH SCAN TOOL, IN THE SIR SERVICE PROCEDURE

#### MODELS: 1992-93 CADILLAC DEVILLE, FLEETWOOD, SIXTY SPECIAL

PLEASE UPDATE THE SUPPLEMENTAL INFLATABLE RESTRAINT (SIR) SERVICE PROCEDURE IN SECTION 9J-A-29 OF THE SERVICE MANUAL TO REFLECT THE REVISED ATTACHED CHART. THE BOLDED BOXES WITHIN THE CHART INDICATE THE CHANGES.

THE "YES/NO" DIRECTIVES IN STEP 3 ARE REVERSED. ALSO THE SUFFIX "A" SHOULD BE ADDED TO J35616 AT THE TOP OF THE CHART.

FIGURES: 0 ATTACHMENTS: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.