For 1990-2009 cars

# SMU - SECTION 6E - ENGINE CONTROLS - AND 6E3

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E-ENGINE CONTROLS- AND 6E3 - DRIVEABILITY AND EMISSIONS - REVISED DTC P0101 TO REVERSE THE YES AND NO BOXES FOR STEP THREE

#### MODELS: 1996 BUICK ROADMASTER 1996 CADILLAC FLEETWOOD 1996 CHEVROLET CAPRICE, CORVETTE, IMPALA SS 1996-97 CHEVROLET CAMARO 1996-97 PONTIAC FIREBIRD WITH 4.3L AND 5.7L ENGINES (VINS W, P - RPOS L99, LT1)

THIS BULLETIN IS BEING ISSUED TO INFORM THE TECHNICIAN OF AN ERROR IN THE SERVICE INFORMATION LISTED IN DTC P0101. THE YES AND NO BOXES FOR STEP THREE NEED TO BE REVERSED.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.