NEW BOTTOM PAN AND COATING CELLULOSE GASKET. Cadillac Limousine 1986

For 1990-2009 cars

# NEW BOTTOM PAN AND COATING CELLULOSE GASKET

#### MODELS AFFECTED: 1985-1988 DE VILLES AND FLEETWOODS 1986-1988 ELDORADOS AND SEVILLES

A new transaxle bottom pan and gasket designed to reduce the chance of crushing or splitting the gasket during installation is now available for service. The revised design uses a continuous raised rib on the pan, refer to Figure 1, and a latex-coated cellulose gasket.

- When replacing the bottom pan on all 1985-1988 THM 440-T4 transaxles, use the service package listed below.

P/N Contents --- -------- 8662942 Transaxle Bottom Pan Package (1)Transaxle bottom pan gasket (stiff, black latex-coated cellulose) (1)Transaxle bottom pan (raised rib) (1)Chip collector magnet

#### NOTE: If the previous pan is used with the new gasket or the new pan is used with a cork gasket, fluid leaks may develop.

- When replacing the bottom pan gasket on all 1985-1988 THM 440-T4 transaxles built after January 4, 1988 (Julian Date 005), use P/N 8668028.

- Overhaul Seals & Gaskets Package, P/N 8646975, and Overhaul Repair Complete Package, P/N 8646976, include the new latex-coated cellulose gasket and the previous design latex-coated cork gasket.

Refer to the THM 440-T4 Automatic Transaxle Unit Repair Table Of Contents for bottom pan and gasket service information.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.