SIX-WAY SEAT ADJUSTER MOVEMENT REPLACE TORQUE TUBE SPRING. Cadillac Limousine 1985

For 1990-2009 cars

# SIX-WAY SEAT ADJUSTER MOVEMENT REPLACE TORQUE TUBE SPRING

#### MODELS AFFECTED: 1985 FWD DEVILLES AND FLEETWOODS

1985 "C" cars equipped with Hancock seat adjusters may experience a rocking movement between the upper and lower six-way seat adjuster channels on either the driver's or passenger's side. The Hancock adjuster may be identified by its long, horizontal jackscrew (refer to Figure 1). To repair this condition, replace the existing torque tube springs.

Replace the torque tube spring for the driver's outer front and passenger's inner front with P/N 20300208. For the driver's inner front and rear, and passengers outer front and rear, use P/N 20369775.

To replace the torque springs, use the following procedure:

1. Remove seat adjuster assembly from seat frame.

2. Using a locking type pliers and a large screwdriver, as shown in Figure 1, carefully turn spring until hook end of spring can be pried from spring stop.

3. To install spring, use care and reverse removal procedure. If hook end of spring will not clear spring stop, it will be necessary to only partially engage spring in the torque tube slot. After engagement with stop, spring must be tapped into full engagement in slot on end of torque tube.

For warranty purposes, use labor Operation No. C6050 at .7 hour for passenger side or C6051 at .7 hour for driver side.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.