REPLACEMENT OF DISCOLORED BODY SIDE MOLDINGS- NEW PART NUMBER. Cadillac Limousine 1987

For 1990-2009 cars

# REPLACEMENT OF DISCOLORED BODY SIDE MOLDINGS- NEW PART NUMBER

REPLACEMENT OF DISCOLOURED BODY SIDE MOULDINGS

#### VEHICLES AFFECTED: 1985-1988 DE VILLE AND FLEETWOOD -----------------

Some 1985-1987 De Villes and Fleetwoods may exhibit a condition of discoloured body side mouldings. New mouldings with increased ultraviolet stabilizers are being used in production and service to repair this condition. The part numbers listed in Figure 1 should be used to service 1985-1987 vehicles and can be used for service on 1988 vehicles.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.