Automatic Transmission Components. Chevrolet Brazil Blazer 1997

For 1990-2009 cars

## Automatic Transmission Components 4.3L

#### CompLoc S/T (4.3L) truck

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
1-2 Shift Solenoid Valve (1-2 SS Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
2-3 Shift Solenoid Valve (2-3 SS Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
3-2 Shift Solenoid Valve Assembly | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Automatic Transmission Fluid Pressure Manual Valve Position Switch (TFP Val. Position Sw.) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Automatic Transmission Fluid Temperature Sensor (TFT Sensor) | In the TFP Val. Position Sw. | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
4 Wheel Drive Indicator Assembly | In the center floor console | 8A-201-41 Fig 42 | -- | --
Front Axle Switch | On the front axle, to the right of the differential | 8A-201-5 Fig 6 | 8A-202-37 | --
IP Fuse Block | LH side of the IP | 8A-201-49 Fig 50 | 8A-11-0 | --
Pressure Control Solenoid Valve (PC SOL. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Selector Quadrant Switch | In the center floor console | 8A-201-41 Fig 42 | -- | --
TCC Brake and Cruise Control Switch | Below LH side of IP, mounted on the brake pedal support | 8A-201-40 Fig 41 | 8A-202-96 | --
Torque Converter Clutch Pulse Width Modulation Solenoid Valve (TCC PWM Sol. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Torque Converter Clutch Solenoid Valve (TCC Sol. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Transfer Case Select Switch | Front center of the IP above the radio | 8A-201-45 Fig 46 | 8A-202-99 | --
Transfer Case Shift Control Module | Behind the center of the IP | 8A-201-53 Fig 54 | 8A-202-98 | --
Vehicle Control Module (VCM) | RH side of the engine compartment | 6 - Engine Controls | -- | --
C1 (32 cavities) | Engine harness to VCM, RH side of the engine compartment | -- | 6 - Engine Controls | --
C2 (32 cavities) | Engine harness to VCM, RH side of the engine compartment | -- | 6 - Engine Controls | --
C3 (32 cavities) | Engine harness to VCM, RH side of the engine compartment | -- | 6 - Engine Controls | --
C4 (24 cavities) | Engine harness to VCM, RH side of the engine compartment | -- | 6 - Engine Controls | --
Vehicle Speed Sensor (VSS) | Rear RH side of the transmission | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
C100 (15 cavities) | Engine to front of dash harness, LH rear of the engine compartment, above the brake booster | 8A-201-25 Fig 26 | 8A-202-109 | --
C114 | Engine to VSS jumper harness, rear RH side of the transmission | -- | -- | --
C149 | Front of dash to front axle switch jumper harness, near the front axle, right of the differential | -- | -- | --
C175 | Engine to front of dash harness, LH rear of the engine compartment, above the brake booster | -- | -- | --
C200 (56 cavities) | IP to front of dash harness, behind RH side of the IP | 8A-201-44 Fig 45 | 8A-202-119 | --
C217 (16 cavities) | Engine to IP extension harness, behind RH side of the IP | 8A-201-44 Fig 45 | 8A-202-133 | --
G104 | Rear of the LH cylinder head | 8A-201-12 Fig 13 | -- | --
P100 | LH rear of the engine compartment, on the cowl | 8A-201-24 Fig 25 | -- | --
P101 | RH rear of the engine compartment, on the cowl | -- | -- | --
S110 | Engine harness, about 6 cm from the dash harness | -- | -- | --
S115 | Engine harness, about 4 cm from the dash harness breakout | -- | -- | --
S120 | IP extension harness, about 33 cm from pass-through P100 | -- | -- | --
S116 | Engine harness, about 13 cm from the fuel injector breakout | -- | -- | --
S203 | IP harness, about 18 cm from the instrument cluster connector breakout | 8A-201-54 Fig 55 | -- | --
S214 | Front of dash harness, about 25 cm right of pass-through P100 | 8A-201-39 Fig 40 | -- | --
S222 | IP harness, about 6 cm from the relay center breakout | 8A-201-54 Fig 55 | -- | --
S227 | Front of dash harness, about 18 cm from the TCC brake and cruise control switch breakout | 8A-201-40 Fig 41 | -- | --
S230 | Front of dash harness, about 6 cm right of the steering column harness breakout | 8A-201-37 Fig 38 | -- | --
S232 | Front of dash harness, about 19 cm right of the steering column harness breakout | 8A-201-37 Fig 38 | -- | --
S237 | IP harness, about 4 cm left of the cigarette lighter breakout | 8A-201-54 Fig 55 | -- | --
S242 | Front of dash harness, about 37 cm right of the steering column harness breakout | 8A-201-37 Fig 38 | -- | --
S243 | Front of dash harness, about 10 cm into the 4WD indicator breakout | 8A-201-37 Fig 38 | -- | --