GM GOODWRENCH 350 DIESEL ENGINE P/N'S. Chevrolet Celebrity 1982

For 1990-2009 cars

# GM GOODWRENCH 350 DIESEL ENGINE P/N'S

#### Model and Year 1978-81 "C" TRUCK, 1980-84 IMPALA AND CAPRICE, 1982-83 MALIBU, 1982-84 MONTE CARLO, AND 1983-84 EL CAMINO

#### TO: ALL CHEVROLET DEALERS

This replaces Chevrolet Dealer Service Bulletin supplement 83-I-94 dated September, 1984, which should be destroyed. This reissue aligns passenger and truck by model, year and appropriate labor time to each.

The labor time allowance for the replacement of a GM Goodwrench 350 diesel engine has been revised as noted below. The revised time allowances are effective immediately and will appear in the September printing.

#### LABOR TIME ALLOWANCES:

1980-84 Impala/ Caprice/Malibu/ Labor Operation Monte Carlo 1978-81 "C" Number El Camino Truck Models ------ --------- ------------

066100 - 7.7

J1840 8.5 7.7

#### Add:

---- With Cruise Control .1 .1 With Air Conditioning .4 .5 Replace Governor Weight Retaining Ring (if required) .7 .7

Includes drain and refill engine oil (if required) and coolant. Check injection pump governor weight retainer ring. Make all necessary adjustments including timing. Also includes time to transfer all required parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.