LUGGAGE CARRIER NOISE INCORRECT INSTALLATION. Chevrolet Celebrity 1984

For 1990-2009 cars

# LUGGAGE CARRIER NOISE INCORRECT INSTALLATION

#### Model and Year 1984 CELEBRITY

Windnoise caused by a roof luggage carrier can be eliminated by replacing the current cross rails with newly released parts.

New Cancelled P/N P/N Part Name ---- --- --------- 14086340 14044206 Cross rail assembly - roof luggage carrier (bright) 2 required per vehicle (base "A" car).

14086342 14079695 Cross rail assembly - roof carrier luggage (black) 2 required per ve- hicle (Eurosport).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.