DOES NOT MEET STATE EMISSION INSPECTION - PROCEDURE. Chevrolet Celebrity 1984

For 1990-2009 cars

# DOES NOT MEET STATE EMISSION INSPECTION - PROCEDURE

#### Model and Year: 1984 Celebrity, Camaro and Citation with LR8 (VIN Code R and S) LQ9 (VIN Code Z) 2.5L Engines and Manual Transmission

#### TO: ALL CHEVROLET DEALERS

If any 1984 Celebrity, Camaro or Citation with 2.5L engines and manual transmissons experience difficulty meeting the hydro-carbon idle exhaust emission requirements of state inspection maintenance test programs, and normal shop manual procedures do not correct the problem, the following list of service PROMS are available from GMWDD.

Service PROM Model Engine Transmission Axle ---- ----- ------ ------------- ---- 1227882 Chevrolet Citation 2.5L(LR8) 4-Spd.Manual(M19) 3.65 (CY5) Chevrolet Celebrity 2.5L(LR8) 4-Spd.Manual(M19) 1227884 Cbevrolet Camaro 2.5L(LQ9) 5-Spd.Manual(ML3)

1227883 Chevrolet Camaro 2.5L(LQ9) 4-Spd.manual(MO8) 1227885 Chevrolet Citation 2.5L(LR8) 4-Spd.Manual(MY8) 3.32 (F25)

Use applicable labor time and operation numbers.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.