ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART. Chevrolet Celebrity 1986

For 1990-2009 cars

# ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART

#### VEHICLES AFFECTED: 1987 THM 125C - WINDSOR BUILT MODELS (PDC, CTC, CXC, CPC, PSC, CBC) A, J AND P CARS

Windsor built 1987 THM 125C Transaxles built between February 18th and February 25th, 1987 (Julian Dates 049 thru 056) were built with suspect torque converter clutch (TCC) solenoids which could cause a condition of engine stalling while shifting into reverse or drive after engine restart.

If a vehicle equipped with the above mentioned transaxles exhibit this condition, replace the torque converter clutch (TCC) sblenoid. Refer to the appropriate transaxle manual for transaxle identification information and proper replacement procedures.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.