POWER STEERING LEAK REPLACE HOSE ASSEMBLY. Chevrolet Celebrity 1987

For 1990-2009 cars

# POWER STEERING LEAK REPLACE HOSE ASSEMBLY

#### Model and Year: 1987 CELEBRITY WITH 2.5L (VIN R) ENGINE

Some 1987 Celebrity models with 2.5L engines may experience a slight leakage from the power steering pressure hose connector assembly at the connection of the hose to the power steering pump.

If this condition is experienced replace the complete power steering pressure hose with service power steering hose assembly P/N 26012610. Follow the service procedure published in the Celebrity service manual.

Relocation of the air conditioning switch assembly and associated wiring will be required. Refer to Figures 1 and 2 .

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.