125-125C ROUGH NEUTRAL TO DRIVE, NEW CLUTCH WAVE PLATE. Chevrolet Celebrity 1983

For 1990-2009 cars

# 125-125C ROUGH NEUTRAL TO DRIVE, NEW CLUTCH WAVE PLATE

#### Model and Year 1982-84 CAVALIER, CITATION AND CELEBRITY

Some 1982-84 THM 125/125C transmission may exhibit a rough neutral to drive gear engagement condition.

Beginning December, 1983, a new forward clutch wave plate, P/N 8652126, went into production.

When servicing any 1982-84 model THM 125/125C transmission for this rough neutral to drive conditon order part number 8652126. Refer to the service manual for removal and replacement of the forward clutch wave plate.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.