REVISED POWER STEERING GEAR UPPER THRUST BEARING SPACER. Chevrolet Chevette 1980

For 1990-2009 cars

# REVISED POWER STEERING GEAR UPPER THRUST BEARING SPACER

THE METHOD OF MANUFACTURING THE POWER STEERING GEAR UPPER THRUST BEARING SPACER HAS BEEN REVISED FOR ALL MODEL YEARS AND SERIES STEERING GEARS. (800,808 AND 605). THE UPPER THRUST BEARING SPACER IS BEING MANUFACTURED WITH A SPLIT(FIG. 1). THE THRUST BEARING SPACER SHOULD NOT BE REPLACED BECAUSE OF THE SPLIT. ALL FUTURE SERVICE PARTS WILL BE OF THE SPLIT SPACER TYPE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.