CHECK ENGINE LAMP DRIVER BOARD LOCATION INFORMATION. Chevrolet Citation 1981

For 1990-2009 cars

# CHECK ENGINE LAMP DRIVER BOARD LOCATION INFORMATION

Chart No. 5, Figure 6E-27 page 6E-21 of the 1982 Service Manual refers to the remote check engine lamp driver circuit board. In prior model years, this function was performed internally in the ECM. This circuit board is located on the IP harness near the ECM. Figure 1 shows the replacement of the circuit board. Make note of this in your 1982 Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.