Lever, Handle, Panel, Switch - Outboard Driver Seat. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications. Refer to Fastener Tightening Specifications (Link disabled for test).
1 | Lever, Driver Seat Lumbar Support Actuator Tip: The lever is a press fit design.
2 | Clip, Driver Seat Recliner Handle Spring
3 | Handle, Driver Seat Recliner
4 | Screw, Driver Seat Cushion Outer Finish Panel Tighten: to 2.5 N·m (22 lb in).
5 | Knob , Driver Seat Adjuster Switch
6 | Panel, Driver Seat Cushion Outer Finish Tip: Slide the panel toward the rear of the vehicle. Remove the panel from the recliner end first.
7 | Bolt, Seat Belt Anchor Tighten: to 32 N·m (24 lb ft).
8 | Switch, Driver Seat Heater
9 | Switch, Driver Seat Adjuster