For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Lower Ball Joint Nut

- First Pass

40 N·m

30 lb ft

- Second Pass

Plus 135°

Lower Control Arm to Frame Nut | 165 N·m | 122 lb ft
Shock Absorber Lower Nut | 28 N·m | 21 lb ft
Shock Absorber Top Nut | 42 N·m | 31 lb ft
Shock Absorber Upper Nut | 47 N·m | 35 lb ft
Stabilizer Shaft Link Nuts | 72 N·m | 53 lb ft
Stabilizer Shaft Mounting Bracket Bolts | 55 N·m | 41 lb ft
Toe Link to Frame Nut | 100 N·m | 74 lb ft
Toe Link to Knuckle Nut

- First Pass

30 N·m

22 lb ft

- Second Pass

Plus 150°

Upper Ball Joint Nut

- First Pass

30 N·m

22 lb ft

- Second Pass

Plus 150°

Upper Control Arm to Frame Bolt | 110 N·m | 81 lb ft
Wheel Bearing/Hub Assembly Mounting Bolts | 115 N·m | 85 lb ft
Wheel Speed Sensor Wiring Harness Bracket Bolt | 10 N·m | 89 lb in