For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Brake Pedal Position Sensor Assembly

#### Procedure

Disconnect the electrical connector.

2 | Brake Pedal Position Sensor Bolt Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Calibrate the position sensor. Refer to Brake Pedal Position Sensor Calibration.
2. Do not reuse the position sensor or bolt. Always use a new sensor and bolt.

Tighten
2 N·m (18 lb in)