For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Driver or Passenger Seat Replacement .

1 | Power Seat Motor Clip
2 | Power Seat Motor Pin
3 | Power Seat Motor Pivot Rolled Pin Tip Use a small punch to remove the rolled pin from the motor assembly and bracket.
4 | Power Seat Motor Assembly

#### Procedure

Disconnect the electrical connector and remove the motor assembly.