For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the folding top.

1 | Folding Top Front Latch Handle Cover
2 | Folding Top Front Latch Handle Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 21 N·m (16 lb ft)
3 | Folding Top Front Latch Handle
4 | Folding Top Front Latch Handle Screw Tighten 5 N·m (44 lb in)
5 | Folding Top Front Latch