For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .

1 | Inflatable Restraint Steering Wheel Module Assembly Caution: Refer to SIR Caution in the Preface section. Caution: Refer to SIR Inflator Module Handling and Storage Caution in the Preface section.

#### Procedures

1. Insert a small blunt ended punch, or equivalent tool, through the access openings on the left and right of the steering wheel.
2. Push the spring fastener inward to release the steering wheel inflator from the steering wheel.