For 1990-2009 cars

Number | Description | Material | Procedure
--- | --- | --- | ---
1 | Front Impact Bar | High Strength Low Alloy Steel | Front Bumper Impact Bar Bracket Replacement
2 | Hood Hinge Bracket | High Strength Low Alloy Steel | Hood Hinge Bracket Replacement
3 | Radiator Lower Support | Mild Steel | Radiator Lower Support Replacement
4 | Battery Tray | High Strength Low Alloy Steel | Battery Tray Replacement
5 | Windshield Panel Upper | Mild Steel | Windshield Frame Header Front Panel Replacement
6 | Windshield Panel Replacement - Lower | Mild Steel | Windshield Lower Panel Replacement
7 | Rear Compartment Panel | Sheet Molded Compound | Rear Compartment Panel Replacement
8 | Rear End Panel | Mild Steel | Rear End Panel Replacement
9 | Quarter Panel Filler | Mild Steel | Quarter Panel Filler Replacement - Lower
10 | Rear Impact Bar | Ultra High Strength Steel | Rear Bumper Impact Bar Replacement
11 | Rear Rail End | Dual Phase Steel | Rear Rail End Replacement
12 | Quarter Panel | Mild Steel | Quarter Outer Panel Replacement
13 | Rear Rail Section | Dual Phase Steel | Rail Replacement - Rear Section
14 | Floor Panel | Mild Steel | Floor Panel Replacement
15 | Front Hinge Pillar Reinforcement | Mild Steel | Front Hinge Pillar Body Reinforcement Replacement
16 | Front Hinge Pillar | High Strength Low Alloy Steel | Front Hinge Pillar Body Replacement
17 | Front Rail Section | Dual Phase Steel | Rail Replacement - Front Section
18 | Front Suspension Crossmember | High Strength Low Alloy Steel | Front Suspension Crossmember Replacement
19 | Front Rail End | Dual Phase Steel | Front Rail End Replacement