For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the tires and wheels. Refer to Tire and Wheel Removal and Installation .

1 | Nut, Stabilizer Shaft Link Retaining (Qty: 2) Tighten 72 N·m (53 lb ft)
2 | Link, Stabilizer Shaft