For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Assist Handle | 6 N·m | 53 lb in
Front Side Door Armrest Pull Cup Bolt | 2 N·m | 18 lb in
Front Side Door Inside Handle Bolt | 2 N·m | 18 lb in
Front Side Door Trim Bolt | 2.5 N·m | 22 lb in
Front Side Door Trim Bracket Bolt | 2.5 N·m | 22 lb in
Front Side Door Window Switch Bezel Screw | xx N·m | xx lb in
Rear Side Door Armrest Pull Cup Bolts | 2 N·m | 18 lb in
Rear Side Door Inside Handle Bolt | 2 N·m | 18 lb in
Rear Side Door Trim Bolt | 2.5 N·m | 22 lb in
Rear Side Door Trim Bracket Bolt | 2.5 N·m | 22 lb in
Rear Side Door Window Switch Bezel Screw | xx N·m | xx lb in
Sunshade Bolt | 3 N·m | 27 lb in
Sunshade Support Bolt | 3 N·m | 27 lb in