For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the mobile telephone control module. Refer to Mobile Telephone Control Module Replacement.
3. Disconnect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Theft Deterrent Module

#### Procedure

1. Disconnect wiring connectors as needed.
2. Unclip the module from the bracket.