For 1990-2009 cars

#### Special Tools

EN-48250 Installer-Crankshaft Front Oil Seal

For equivalent regional tools, refer to Special Tools.

1. Install a NEW oil pump drive shaft seal.
2. Use the EN-48250 installer (1) to install the oil pump drive shaft seal (2).

Note: While installing the oil pump drive shaft seal (1) to the oil pump housing (2) it is importantly that the oil pump drive shaft seal concisely at the cylinder head fits.

3. Install the oil pump drive shaft seal (1).