For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle's RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
01K | TRIM COLOR SEAT - BRICK
01O | TRIM COLOR SEAT - V DK PEWTER
01S | TRIM COLOR SEAT - MED TITANIUM
01Y | TRIM COLOR SEAT - SONIC BLUE
1A1 | TRIM COLOR DR PANEL - SONIC BLUE
1AQ | TRIM COLOR DR PANEL - V DK PEWTER
1BF | TRIM COLOR DR PANEL - BRICK
4AA | INTERIOR TRIM - JET BLACK
4AQ | INTERIOR TRIM - V DK PEWTER
6Y4 | TIRE AND WHEEL - SPARE - DELETE
A01 | WINDOW TINTED - ALL, SHADED WINDSHIELD
A23 | WINDSHIELD - HEAT REFLECTIVE
A51 | SEAT - FRT BKT, CUSTOM
A62 | SEAT RR - FIXED SEAT BACK
A64 | SEAT RR - SPLIT, FOLDING, 40/60
ADL | RESTRAINT SYSTEM - SEAT, INFLATABLE, DRIVER AND PASS, SINGLE STAGE
AEC | WINDOW - POWER OPERATED, DRIVER EXPRESS DOWN
AED | WINDOW - POWER OPERATED, PASSENGER, EXPRESS DOWN
AEQ | WINDOW - POWER OPERATED, RR DRS, EXPRESS DOWN
AFA | INTERIOR TRIM CONFIG - 1
AFB | INTERIOR TRIM CONFIG - 2
AFC | INTERIOR TRIM CONFIG - 3
AFD | INTERIOR TRIM CONFIG - 4
AFE | INTERIOR TRIM CONFIG - 5
AFF | INTERIOR TRIM CONFIG - 6
AFG | INTERIOR TRIM CONFIG - 7
AFH | INTERIOR TRIM CONFIG - 8
AFI | INTERIOR TRIM CONFIG - 9
AG5 | ADJUSTER PASS ST - MANUAL, 2 WAY
AH3 | ADJUSTER FRT ST - MANUAL, 4 WAY, DRIVER
AH9 | ADJUSTER FRT ST - MANUAL, 2 WAY, DRIVER
AHR | RESTRAINT - HEAD, FRT SEAT, UP/DOWN, FORE/AFT ADJUSTMENT
AJC | RESTRAINT - HEAD, FRT SEAT, UP/DOWN ADJUSTMENT
AJG | RESTRAINT SYSTEM - SEAT, INFLATABLE, DRIVER AND PASS, FRT AND SEAT SIDE, SINGLE STAGE
ASV | EQUIPMENT - SENSOR AIR MOISTURE AND W/S TEMP
ATH | LOCK CONTROL, ENTRY - REMOTE ENTRY, EXTENDED RANGE, PASSIVE ENTRY
AWP | RESTRAINT SYSTEM RR - SEAT BELT, REAR, 2 POINT, CTR, LAP BELT
AXG | WINDOW - POWER OPERATED-EXPRESS DRIVER UP/DOWN
AXJ | VEHICLE TYPE - PASSENGER CAR
AYC | RESTRAINT SYSTEM - SEAT, INFLATABLE, DRIVER AND PASS FRT, SEAT SIDE, ROOF SIDE, SINGLE STAGE
B34 | COVERING FRT - FLOOR MATS, CARPETED INSERT
B35 | COVERING REAR - FLOOR MATS, CARPETED INSERT
B76 | CLUSTER COLOR - INST, BLACK
BAH | EQUIPMENT - SECURITY SYSTEM, IMMOBILIZATION, STEP TWO
BD6 | MOLDING ROOF - BLACK
BTM | SWITCH - ENGINE START, KEYLESS
C32 | HEATER - HEATING/DEFROSTER SYSTEM, REINFORCED, ELECTRIC
C49 | DEFOGGER - RR WINDOW, ELECTRIC
C67 | HVAC SYSTEM - AIR CONDITIONER FRT, ELECTRONIC CONTROLS
C68 | HVAC SYSTEM - AIR CONDITIONER FRT, AUTO, ELECTRONIC CONTROLS
C95 | LAMP - INTR, ROOF, COURTESY AND DUAL READING
CE1 | WIPER SYSTEM - WINDSHIELD, PULSE, MOISTURE SENSITIVE
CF5 | ROOF - SUN, GLASS, SLIDING, ELEC
CW1 | COUNTRY - KOREA
D31 | MIRROR I/S R/V - TILT
D75 | HANDLE O/S DOOR - BODY COLOR
D7A | HANDLE O/S DOOR - BODY COLOR, CHROME STRIP
D91 | HANDLE - O/S, L/GATE, R/CMPT, COLOR
DA1 | ARM REST - RR SEAT, STORAGE
DA2 | ARM REST - RR SEAT, STORAGE, PASS THROUGH
DBU | CONSOLE - FRT COMPT, FLOOR, ARM REST SLIDING
DD8 | MIRROR I/S R/V - LT SENSITIVE
DLU | MIRROR I/S FRT VAN - SUNSHADE, DRIVER, W/O MIRROR, PASS, W/MIRROR AND COVER
DMH | MIRROR I/S FRT VAN - SUNSHADE, DRIVER, W/MIRROR, COVER, ILLUM, PASS, W/MIRROR, COVER
DP6 | MIRROR PROVISIONS - HOUSING, PAINTED
DT4 | ASHTRAY - CIGARETTE LIGHTER
DVA | CLUSTER COLOR - INST, BLACK, BLACK RINGS W/SILVER TOP
DWF | MIRROR O/S - LH AND RH, RC, ELEC, HEAT, AUX WFOV/DRVR, PWRFOLD, CNVX/PASS
DWT | MIRROR O/S - LH AND RH, RC, MANIFOLD, AUX WFOV/DRVR, CNVX/PASS
E3E | HANDLE - O/S, L/GATE, R/CMPT, CHROME
EA1 | POCKET - FRONT SEAT BACK, LH
EA2 | POCKET - FRONT SEAT BACK, RH
EBF | TRIM SEAT - LEATHER, MERIDIAN
EBG | TRIM SEAT - CLOTH, FLAT WOVEN
EBJ | TRIM SEAT - CLOTH, MESH
FX1 | RATIO - TRANSAXLE FINAL DRIVE 3.94
FX3 | RIDE AND HANDLING - AUTOMATIC ELECTRONIC CONTROLLED
FX6 | RATIO - TRANSAXLE FINAL DRIVE 3.87
FXF | RATIO - TRANSAXLE FINAL DRIVE 3.26
FXQ | RATIO - TRANSAXLE FINAL DRIVE 2.29
GAR | PRIMARY COLOR - EXTERIOR, CARBON FLASH MET (G)
GCB | PRIMARY COLOR - EXTERIOR, CARBON FLASH MET (G) PRIMARY COLOR - EXTERIOR, GALAXY WHITE (G)
GCT | PRIMARY COLOR - EXTERIOR, MOROCCAN BLUE MET (G)
GCV | PRIMARY COLOR - EXTERIOR, PEWTER GREY MET(G)
GCW | PRIMARY COLOR - EXTERIOR, MISTY LAKE MET (G)
GCY | PRIMARY COLOR - EXTERIOR, POLY SILVER MET(G)
GNA | CHASSIS EQUIP FRONT - STRUT ASM
GNF | CHASSIS EQUIP REAR - REAR AXLE, COMPOUND CRANK
J60 | BRAKE SYSTEM - POWER, FRT AND RR DISC, ABS, 16"
J67 | BRAKE SYSTEM - POWER, FRT AND RR DISC, ABS, 15"
J93 | BRAKE SYSTEM - POWER, FRT DISC, RR DRUM, ABS, 15"
J94 | BRAKE SYSTEM - POWER, FRT DISC, RR DRUM, 15"
JJ2 | BRAKE LINING - BRAKE NOISE AND DUST PERFORMANCE
K60 | GENERATOR - 100 AMP
KA1 | HEATER - SEAT, FRT
KC7 | RECEPTACLE - ELECTRICAL, RR SEAT
KCL | HEATER - DUCT, RR PASS (2ND POSN)
KG9 | GENERATOR - 140 AMP
KTF | KEY - PRIMARY FOLDABLE, ADDITIONAL FOLDABLE
KUA | PLANT CODE - GUNSAN, KOREA
LHD | VEHICLE DRIVE - LEFT HAND DRIVE
LLW | ENGINE - DIESEL, 4 CYL, L4, 2.0L, CRI, SOHC, TURBO, 110 KW,
LXV | ENGINE - GAS, 4 CYL, 1.6L, MFI, DOHC, PT-JV, VARIABLE CAMSHAFT PHASING, 82KW
MDB | MOLDING B/S UPPER - BLACK
MDC | MOLDING B/S UPPER - BRIGHT
MFH | TRANSMISSION - MAN 5 SPD, D16 M/CR
MFV | TRANSMISSION - MAN 5 SPD, D33 SUPER-WIDE, 3.947 1ST, 0.721 5TH
MH7 | TRANSMISSION - AUTO 6 SPD, HMD, X23FHD
MH8 | TRANSMISSION - AUTO 6 SPD, HMD, X23F
MH9 | TRANSMISSION - AUTO 6 SPD, HMD, X24F
N33 | STEERING COLUMN - TILT TYPE
N34 | STEERING WHEEL - LEATHER, 3 SPOKES
N37 | STEERING COLUMN - TILT, TELESCOPING
N40 | STEERING - POWER, NON-VARIABLE RATIO
N45 | STEERING WHEEL - 3 SPOKES
N92 | COVER, WHEEL - BOLT-ON
NQU | EMISSION SYSTEM - KOREAN, ULEV
NT4 | EMISSION SYSTEM - EEC 05
PWL | WHEEL - 15 X 6.5, STEEL, DESIGN1 TBD GLOBAL DELTA
Q0D | TIRE ALL - P215/50R17-90H BW R/ST TL AL3
Q0E | TIRE ALL - P225/50R17-93V BW R/ST TL AL3
Q0L | TIRE ALL - P205/60R16-91V BW R/ST TL AL3
QRV | TIRE ALL - P205/65R15-92H BW R/ST TL AL3
T39 | LAMP - TURN SIGNAL, AUX
T3U | LAMP - FRT FOG
T4A | HEADLAMPS - HALOGEN
T68 | BATTERY - LN4, FLA, 12V, 80AH, 600 CCA
T74 | HEADLAMPS CONTROL - AUTOMATIC, DELAY
T83 | HEADLAMPS CONTROL - AUTOMATIC ON-OFF
TM7 | BATTERY - LN2, FLA, 12V, 60AH, 438 CCA
TPV | GRILLE - RADIATOR, BLACK, W/CHROME BAR
TR8 | REFLECTOR - WARNING, DISABLED VEHICLE
TS6 | LAMP - STOP, HIGH LEVEL
TTO | RADIO EQUIPMENT - COOLING SYSTEM
TTX | RADIO EQUIPMENT - AUX CONNECTOR (LINE IN)
U07 | HORN - FANFARE
U77 | ANTENNA - RR WINDOW, RADIO
UAG | INFOTAINMENT DISPLAY - GRAPHIC INFO DISPLAY (GID), VAR 1
UD7 | SENSOR INDICATOR - REAR PARKING ASSIST
UDB | DISPLAY INSTRUMENT - DRIVER INFO ENHANCED (SEGMENTED)
UDK | INFOTAINMENT DISPLAY - COLOR INFO DISPLAY (CID) 7", QVGA
UEC | SENSOR INDICATOR - AUTOMATIC AIR RECIRCULATION
UH0 | INDICATOR - SEAT BELT WARNING , LH
UKA | RADIO - AM/FM STEREO, CD-ROM, CAF, MUSIC NAVIGATOR (KOREA VERSION)
UQF | SPEAKER SYSTEM - STANDARD AUDIO
UQG | SPEAKER SYSTEM - ENHANCED AUDIO WITH AMPLIFIER
UTJ | THEFT DETERRENT - ELECTRICAL, UNAUTHORIZED ENTRY
UV8 | TELEPHONE - PROVISIONS FOR MOBILE
UYL | RADIO - AM/FM STEREO, CDX-ROM, CAF, MUSIC NAVIGATOR (KOREA VERSION)
UYR | RADIO - AM/FM STEREO, NAV, DVD-ROM, CAF, USB, (KOREA VERSION)
UZ6 | SPEAKER SYSTEM - 6, PREMIUM
VK8 | HOLDER - EYEGLASSES
VNF | ISOLATOR - BATTERY
VTW | COMPARTMENT - STOWAGE, I/P, W/LID
VTX | COMPARTMENT - STOWAGE, I/P, WO/LID
VWC | PANEL CENTER - INSTRUMENT, HIGH GLOSS BLACK
VY7 | KNOB - TRANS CONT LEVER, LEATHER
W1D | CONTROL - STEERING WHEEL, RADIO AND PHONE, REDUNDANT CONTROLS (DO NOT USE AFTER 2009, USE UC3)
W1Y | CONTROL - STEERING WHEEL, RADIO, REDUNDANT CONTROLS
WQS | WHEEL - 16 X 6.5, ALUMINUM, DESIGN 17 TBD GLOBAL DELTA
WQX | WHEEL - 17 X 7, ALUMINUM, DESIGN 19 TBD GLOBAL DELTA
WTR | KIT, TIRE - TIRE REPAIR
Z1F | IDENTIFICATION - SPEEDOMETER KILOMETER