For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Always connect or disconnect the wiring harness connector from the EBCM/EBTCM with the ignition switch in the OFF position. Failure to observe this precaution could result in damage to the EBCM/EBTCM.

#### Preliminary Procedure

Remove the BPMV from BPMV bracket. Refer to Brake Pressure Modulator Valve Bracket Replacement.

1 | Electronic Brake Control Module Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten XX N·m (XX lb in)
2 | Brake Pressure Modulator Valve
3 | Electronic Brake Control Module