For 1990-2009 cars

#### Special Tools

DT-527-A Adjuster

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the transmission control lever trim cover. Refer to Automatic or Manual Transmission Control Lever Trim Cover Replacement.
2. Remove the front floor console storage tray. Refer to Front Floor Console Storage Tray Replacement.
3. Remove the shift lever and selector lever cable adjust locks (1).
4. Lock the transmission control with DT-527-A adjuster (1).
5. Lock the shift control lever at the transmission.
6. Pull the shift control lever (1) upwards (arrow) and attach DT-527-A adjuster (2) to the shift control lever.

### Installation Procedure

1. Install the shift lever and selector lever cable adjust locks (1).
2. Remove the DT-527-A adjuster from the transmission control.
3. Remove the DT-527-A adjuster from the shift control lever.
4. Install the front floor console storage tray. Refer to Front Floor Console Storage Tray Replacement.
5. Install the transmission control lever trim cover. Refer to Automatic or Manual Transmission Control Lever Trim Cover Replacement.