For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Input Speed Sensor Connector
2 | Output Speed Sensor Connector
3 | Shift Position Switch Connector
4 | Control Valve Body Cover Wiring Connector Hole Seal Tip Do not re-use the valve body cover wiring connector hole seal.
5 | Control Valve Body Cover Gasket Tip Do not re-use the valve body cover gasket.
6 | Control Valve Body Cover
7 | Control Valve Body Cover Bolts M6 x 30 (Qty: 13) Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (106 lb in)