For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Fender Bolt | 8 N·m | 71 lb in
Front Fender Bracket Bolt | 9 N·m | 80 lb in
Front Side Door Check Link Bolt | 25 N·m | 19 lb ft
Front Side Door Check Link Nut | 9 N·m | 80 lb in
Front Side Door Hinge Bolt | 25 N·m | 19 lb ft
Headlamp and Front Bumper Fascia Mount Panel Bolt | 22 N·m | 17 lb ft
Hood Hinge Bolt | 26 N·m | 20 lb ft
Hood Hinge Reinforcement Nut | 26 N·m | 20 lb ft
Rear Compartment Lid Hinge Bolt | 9 N·m | 80 lb in
Rear Side Door Check Link Bolt | 25 N·m | 19 lb ft
Rear Side Door Check Link Nut | 9 N·m | 80 lb in
Rear Side Door Hinge Bolt | 25 N·m | 19 lb ft