For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.

1 | Disconnect Electric Connector Tip The graphic shows the heater and air conditioning evaporator and blower module without instrument panel compartment assembly for better clarity.
2 | Air Conditioning Refrigerant Temperature Sensor - Left Side Tip Turn the air conditioning refrigerant temperature sensor.