For 1990-2009 cars

Application | Ref. No. | Quantity | Specification
--- | --- | --- | ---
Metric | English
Case Extension to Case Assembly | 34 | 6 | 50 N·m | 37 lb. ft.
Control Solenoid Valve Assembly and Control Valve Lower Body Assembly to Control Valve Upper Body Assembly | 310 | 6 | 8 N·m | 71 lb. in
Control Solenoid Valve Assembly and Control Valve Lower Body Assembly to Control Valve Upper Body Assembly | 309 | 10 | 8 N·m | 71 lb. in
Control Solenoid Valve Heat Sink to Valve Body | 312 | 2 | 8 N·m | 71 lb. in
Control Valve Upper Body Assembly to Control Valve Lower Body Assembly | 301 | 12 | 8 N·m | 71 lb. in
Control (with Body and Valve) Valve Assembly to Case Assembly | 22 | 6 | 8 N·m | 71 lb. in
Fluid Pan Assembly to Case Assembly | 30 | 18 | 9 N·m | 80 lb. in
Fluid Pump Cover Assembly to Torque Converter Housing | 231 | 13 | 11 N·m | 97 lb. in
Input and Output Speed Sensor Assembly to Control Valve Upper Body Assembly | 302 | 2 | 12 N·m | 106 lb. in
Line Pressure Test Hole Plug to Torque Converter Housing | 202 | 1 | 11 N·m | 97 lb. in
Manual Shaft Detent Assembly to Valve Body | 23 | 1 | 12 N·m | 106 lb. in
Torque Converter Housing Assembly to Case Assembly | 3 | 9 | 72 N·m | 53 lb. ft.
* Reference number refers to the component callout number in Disassembled Views