For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Torque Converter Cover Bolt Tighten 10 N·m (89 lb. in).
2 | Torque Converter Cover Tip Remove the starter. Refer to Starter Motor Replacement.
3 | Torque Converter Cover Bolt Tighten 10 N·m (89 lb. in).
4 | Torque Converter Cover