For 1990-2009 cars

Component | Circuit Number | Wire Color* | Inline Connector Pin | Resistance at 20°C (68°F) | Resistance at 70°C (158°F) | Resistance to Ground - Transmission Case
--- | --- | --- | --- | --- | --- | ---
1-2 Shift Solenoid Valve | 1525 | WH | 17 | 15.0-17.0 ohms | 17.9-20.3 ohms | Greater than 50Kohms
1222 | BK | 14
2-3 Shift Solenoid Valve | 1525 | WH | 17 | 15.0-17.0 ohms | 17.9-20.3 ohms | Greater than 50Kohms
1223 | BU | 9
4-5 Shift Solenoid Valve | 1525 | WH | 17 | 15.0-17.0 ohms | 17.9-20.3 ohms | Greater than 50Kohms
898 | GY | 5
Pressure Control Solenoid Valve | 1228 | GN | 13 | 3.5-4.6 ohms | 4.2-5.5 ohms | Greater than 50Kohms
1229 | WH | 8
TCC PWM Solenoid Valve | 1525 | WH | 17 | 10.0-11.5 ohms | 11.8-13.6 ohms | Greater than 50Kohms
422 | YE | 20
Input Speed Sensor | 1230 | YE | 18 | 325-485 ohms | 385-575 ohms | Greater than 50Kohms
1231 | WH | 15
Output Speed Sensor | 400 | OG | 1 | 325-485 ohms | 385-575 ohms | Greater than 50Kohms
401 | WH | 3
TFT Sensor | 1227 | RD | 10 | Refer to Transmission Fluid Temperature Sensor Specifications .
2762 | WH | 6
* All wire colors are internal to the transmission.