For 1990-2009 cars

### Removal Procedure

1. Remove the centre console trim plate. Refer to Console Trim Plate Replacement.
2. Using a suitable tool carefully remove the cup holder trim (1) by disengaging the retaining clips.
3. Remove the cup holder mat (1) located at the base of the cup holder.
4. Remove the cup holder to centre console retaining screws (1).
5. Remove the cup holder (4) from the centre console (3) by releasing the retaining lug (2) and lifting upwards.

### Installation Procedure

Important: Listen for an audible click from the retaining lug (2) to confirm correct fitment.

1. Install the cup holder (4) into the centre console (3)

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cup holder to centre console retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the cup holder mat (1).

Important: Listen for an audible click to confirm correct fitment.

4. Install the cup holder trim (1) by firmly engaging the retaining clips.
5. Install the centre console trim plate. Refer to Console Trim Plate Replacement.