For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Steering Column Lower Trim Cover to Steering Column Assembly Retaining Screw | 2 N·m | 18 lb in
Steering Wheel to Steering Column Shaft Retaining Bolt | 45 N·m | 33 lb ft
Ignition Switch to Steering Column Assembly Retaining Screws | 3 N·m | 27 lb in
Steering Column Assembly to Body Retaining Bolts | 22 N·m | 16 lb ft
Steering Column Shaft to Intermediate Steering Shaft Retaining Bolt | 28 N·m | 21 lb ft
Intermediate Steering Shaft to Pinion Shaft Retaining Bolt | 28 N·m | 21 lb ft