For 1990-2009 cars

### Removal Procedure

1. Slide the front of the trim plate (2) away from the centre console extension panel (1).
2. Detach the rear of the trim plate (1) from the centre console (2) by disengaging the retaining clips.
3. Remove the trim plate (1).

### Installation Procedure

1. Engaged the retaining clips at rear of the trim plate (1) to secure it to the centre console (2).
2. Slide the front of the trim plate (2) up into the centre console extension panel (1).
3. Ensure the trim plate is correctly located in the centre console and end panel.