For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result. Important: Clean and inspect all valve components and the valve body. The control valve lower body is replaceable only as an assembly.
1 | Clutch Piston Dam Feed Regulator Valve Train
2 | Clutch Select Solenoid Valve Train
3 | Clutch Select Solenoid Valve Train
4 | Manual Valve
5 | TCC Regulator Apply Valve Train