For 1990-2009 cars

Option Code | Description
--- | ---
12U | Exterior Paint, Odyssey
36U | Exterior Paint, Abalone
463 | Interior Trim, Onyx Leather
51I | Interior Trim, Onyx
64U | Exterior Paint, Karma
80U | Exterior Paint, Phantom
A31 | Power Windows (Front And Rear)
A45 | Function, Exterior Mirror, Heat And Memory
A46 | Adjuster, Easy Entry, Driver and Pasenger
AGA | Adjuster, Passenger Seat 10-Way Power
AGB | Adjuster, Driver Seat 10-Way Power
AHU | Seatbelts, Front, Adjustable Anchorage
AN1 | Seats, Rear, 3 Passenger Fixed Bench (w/ Cup Holders)
AP9 | Convenience Net
ATP | Rear Power Sliding Seat
ATQ | Rear Power Sliding Seat With Massaging
AJ7 | Restraint, Driver, Passenger And Side Inflatable (Airbags)
AKH | Restraint, Driver and Passenger Front Seat Head, Driver Side Active
AQ9 | Seats, Reclining Bucket
AW5 | Seats, Rear Cushion, 3 Position / 2 Bucket
AX2 | Key, Common, Vehicular Unique
AY0 | Restraint Package, Dual Stage Front Airbags, Front Thorax Airbags, Full Length Side Curtain Airbags
B34 | Mats, Carpeted insert, Front
B35 | Mats, Carpeted insert, Rear
B75 | Luggage Compartment Lining, Warning Triangle Provision
B86 | Moulding, Body Side, Body Colour
BMG | Ornamentation, Daewoo
BS2 | Insulation, Acoustic Package
BSI | Identification, Half Model Year Breaking Point
C63 | HVAC Automatic Control (Tri Zone)
CF5 | Sunroof
CE1 | Wiper System, Windshield, Pulse, Moisture and Speed Sensitive
CE9 | Equipment, Additional, Korea
CED | Wipers, 2 Speed Plus Intermittent With Variable Dwell
CHW | Windshield Washer Solvent Heater
CJ2 | HVAC Dual Zone
CW1 | Country, Korea
DB3 | Sunshade, Rear Window, Power
DE8 | Sunshade, Rear Side Window, Manual
DK9 | Exterior Mirrors, Power, Foldable
DNL | Exterior Mirrors - Remote Control, Electric, Heated, Power Folding, Chrome (w/o Puddle Lamp, Blue Glass)
E20 | Interior Door Handles, Body Colour & Chrome Accent
ESA | Assembly Plant, Elizabeth, South Australia
EVF | Equipment, Engine, V6
FE1 | Suspension, Soft Ride
GW6 | Axle, 3.27:1 Final Drive Ratio
GW8 | Axle, 2.92:1 Final Drive Ratio
JL4 | Electronic Stability Program (ESP), Electronic Brake Assist (EBA), Alloytec V6
JL9 | Antilock Brake System (ABS)
K30 | Cruise Control
KA1 | Heater, Front Seats
KA7 | Heater, Front and Rear Seats
KEI | Vehicle Air Purification System
LHD | Vehicle, Left-Hand Drive
LLT | Engine, 3.6 CIDi V6, Alum, 60 Degrees
LY7 | Engine, 3.6 Alloytec V6 4 valve EFI Premium
M82 | Transmission, 5-Speed Automatic 5L40E
MYB | Transmission, 6-Speed Automatic 6L50
N10 | Dual Exhaust
N40 | Power Steering (Non-Variable)
N87 | Wheel, 8.00 X 18 Alloy Road
NP5 | Steering Wheel, Leather Covered With Controls W1Y
NQU | Emissions System, KULEV
NQL | Emissions System, KLEV
P34 | Wheel, Full Size Spare
PFE | Wheel, 7.0 X 17 Alloy Road
QFX | Tyre, 245/45 R18 All Season
QUV | Tyre, 225/55 R17 97V
R1L | Tyre, 245/45 R18 100V
T3U | Lamp, Front Fog
T81 | Tail Lamp Assembly, LED
TT8 | Headlamps, Hid Xenon, Auto Levelling LHD
U32 | Entertainment Package, Rear Seat Player DVD (Only With Premium Sound System And Leather Steering Wheel)
U71 | Antenna, Roof Mounted
UE7 | Digital TV Tuner
UFR | Assist, Front & Rear Park
UVC | Rear View Camera
UV9 | Navigation System, Korean
UWE | Bluetooth Cellular Phone Connectivity
UWQ | Audio System, 220W 6 CD Changer In Head Unit, Preset Equaliser Dsp
V5E | HBD Processing Option
V5Z | Safety Compliance Plate Delete
V7O | Description, Model Year, 2009
VY7 | Knob, Transmission Control Lever, Leather
XQ9 | Badge, Chevrolet
XR5 | Filter, Pollen
XW6 | Metallic Paint
Y9G | Model Conversion, Base
Y9H | Model Conversion, Mid
Y9I | Model Conversion, Upper