For 1990-2009 cars

Table 1: | Door Latch Assembly - LF
Table 2: | Door Latch Assembly - LR
Table 3: | Door Latch Assembly - RF
Table 4: | Door Latch Assembly - RR
Table 5: | Fuel Filler Door Latch
Table 6: | Hood Ajar Switch
Table 7: | Rear Compartment Lid Latch Actuator
Table 8: | Rear Compartment Lid Release Switch

#### Door Latch Assembly - LF

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | -- | -- | Not Used
2 | BN/RD | 0.75 | Door Lock Actuator Unlock Control
3 | GN/WH | 0.75 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | BN/WH | 0.3 | Passenger Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | BK | 0.5 | Ground
9 | -- | -- | Not Used
10 | -- | -- | Not Used

#### Door Latch Assembly - LR

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | -- | -- | Not Used
2 | BN/RD | 0.75 | Door Lock Actuator Unlock Control
3 | GN/WH | 0.75 | Door Lock Actuator Lock Control
4 | BN/WH | 0.3 | Left Rear Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | BK | 0.5 | Ground

#### Door Latch Assembly - RF

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | GY/BK | 0.3 | Right Front Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | BK | 0.5 | Ground
4 | PK | 0.3 | Driver Door Lock Switch Unlock Signal
5 | -- | -- | Not Used
6 | -- | -- | Not Used
7 | BN/RD | 0.75 | Driver Door Lock Actuator Unlock Control
8 | GN/WH | 0.75 | Door Lock Actuator Lock Control
9 | PK/BK | 0.3 | Driver Door Lock Switch Lock Signal
10 | -- | -- | Not Used

#### Door Latch Assembly - RR

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN/WH | 0.3 | Right Rear Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | BK | 0.5 | Ground
4 | -- | -- | Not Used
5 | BN/RD | 0.75 | Door Lock Actuator Unlock Control
6 | GN/WH | 0.75 | Door Lock Actuator Lock Control

#### Fuel Filler Door Latch

Connector Part Information | 2.3 Series
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | GN/WH | 1.25 | Door Lock Actuator Lock Control
2 | BN/RD | 1.25 | Driver Door Lock Actuator Unlock Control

#### Hood Ajar Switch

Connector Part Information | 150 Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BK | 0.3 | Hood Ajar Switch Signal
B | PU | 0.3 | Hood Closed Switch Signal
C | BK | 0.3 | Ground

#### Rear Compartment Lid Latch Actuator

Connector Part Information |
--- | ---
Pin | Wire Color | Wire Size | Function
1 | OG/BK | 0.3 | Rear Compartment Lid Ajar Switch Signal
2 | BU | 0.5 | Rear Compartment Lamp Control
3 | BN/WH | 0.85 | Rear Compartment Lid Release Actuator
4 | BK | 0.85 | Ground

#### Rear Compartment Lid Release Switch

Connector Part Information |
--- | ---
Pin | Wire Color | Wire Size | Function
A | D-BU | 0.3 | Rear Compartment Lid Release Switch
B | BK/WH | 0.5 | Ground