For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Hose to Caliper Banjo Bolt | 35 Nm | 26 lb ft
Brake Master Cylinder Reservoir to Brake Master Cylinder Retaining Screw | 2 Nm | 18 lb in
Brake Master Cylinder to Vacuum Brake Booster Retaining Nut | 10 Nm | 89 lb in
Brake Pedal Assembly to Bulkhead Retaining Nut | 22 Nm | 16 lb ft
Brake Pedal Bracket Assembly to I/P Crossmember Retaining Bolt | 22 Nm | 16 lb ft
Brake Pedal Position Sensor to Brake Pedal Bracket Retaining Bolt | 2 Nm | 18 lb in
Brake Pipe Fitting at Brake Pressure Modulator Valve (BPNV) | 15 Nm | 11 lb ft
Brake Pipe Fitting at Master Cylinder | 15 Nm | 11 lb ft
Brake Pipe Fitting at Brake Hose | 15 Nm | 11 lb ft
Front Brake Hose Inner Wheel House to Frame Retaining Bolt | 9 Nm | 80 lb in
Front Brake Caliper Anchor Plate to Steering Knuckle Retaining Bolt | 60 Nm +120° | 44 lb ft +120°
Intermediate Brake Pipe to Brake Pipe Union | 15 Nm | 11 lb ft
Rear Brake Caliper to Knuckle Retaining Bolt | 110 Nm | 81 lb ft
Vacuum Brake Booster to Bulkhead Retaining Nuts | 22 Nm | 16 lb ft