For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 2-6 and 3-5 Reverse Clutch Hub Thrust Bearing Assembly
2 | 2-6 and 3-5 Reverse Clutch (with Output Carrier Outer Sun Gear Shaft) Hub Assembly
3 | 1-2-3-4 Clutch Hub Thrust Bearing Assembly
4 | 1-2-3-4 Clutch (with Output Carrier Inner Sun Gear Shaft) Hub Assembly
5 | 4-5-6 Clutch Hub Thrust Bearing Assembly
6 | 4-5-6 Clutch (with Output Carrier Shaft and Dampener) Hub Assembly Tip Refer to 4-5-6 Clutch Dampener Overhaul .
7 | Turbine Shaft Thrust Bearing Assembly
8 | 4-5-6 (with Turbine Shaft) Clutch Assembly
9 | Input Sun Gear Thrust Bearing Tip Thrust bearing snaps onto input carrier assembly.
10 | Input Sun Gear Thrust Washer
11 | Input Carrier Assembly
12 | Input Sun Gear
13 | 1-2-3-4 and 3-5 Reverse Clutch Assembly Tip Wiggle the DT 47781 in order to align the 1-2-3-4 and 3-5 reverse clutch plates with the external splines of the 4-5-6 clutch assembly. To verify that the 1-2-3-4 and 3-5 reverse clutch assembly is fully installed, lift up on the turbine shaft. There should not be any noticeable slack.

#### Special Tool

DT 47781 C1234 35R Clutch Assembly Installer