For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section.
1 | Fluid Pan Gasket Important: The fluid pan gasket is reusable. Inspect the gasket to determine if it may be reused. If the gasket is stuck to the case or pan, it should be replaced.
2 | Fluid Pan Assembly.
3 | Fluid Pan Bolts M6 x 20 (Quantity: 18) Tighten 9 N·m (80 lb. in) in sequence shown.