SMU - SECTION 5E1 - ANTILOCK BRAKE SYSTEM REVISED. Geo Prizm 1996

For 1990-2009 cars

# SMU - SECTION 5E1 - ANTILOCK BRAKE SYSTEM REVISED

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 5E1 - ANTILOCK BRAKE SYSTEM REVISED DIAGNOSTIC CIRCUIT CHECK

#### MODELS: 1996 CHEVROLET GEO PRIZM

THIS BULLETIN IS BEING ISSUED TO ADVISE TECHNICIANS OF A REVISION TO THE DIAGNOSTIC CIRCUIT CHECK CHART ON PAGE 5E1-13 OF THE SERVICE MANUAL.

O TERMINAL "25" OF EBCM HARNESS CONNECTOR C1 SHOULD READ: TERMINAL "9" OF EBCM HARNESS CONNECTOR C1.

O TERMINAL "5" OF EBCM HARNESS CONNECTOR C1 SHOULD READ: TERMINAL "1" OF EBCM HARNESS CONNECTOR C1.

O TERMINAL "M" OF ABS DLC SHOULD READ: TERMINAL "9" OF OBD II DLC.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.