AUTOMATIC TRANSAXLE 1ST/REV CLUTCH SNAP RING. Geo Spectrum 1988

For 1990-2009 cars

# AUTOMATIC TRANSAXLE 1ST/REV CLUTCH SNAP RING

#### Model and Year: 1988 R CAR

When overhauling the automatic transaxle assembly, installing a snap ring between the low/reverse brake plate assembly and the brake hub (Figure 1) will make reassembly easier. This snap ring is included in the transaxle overhaul kit, but is not installed in the transmission during initial assembly by the factory.

Part No. Description -------- ----------- 8-94140-795-0 Snap Ring

This is included in:

8-94151-718-0 A/T Repair Kit

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.