DISC BRAKE PAD WEAR REPLACE PADS USING P/N LISTED. Geo Spectrum 1986

For 1990-2009 cars

# DISC BRAKE PAD WEAR REPLACE PADS USING P/N LISTED

#### VEHICLES AFFECTED: 1985-86 'R' CAR

Some of the subject vehicles may exhibit an early wear condition of the front disc brake pad linings. Wear occurring to or beyond the wear sensor in less than 16,000 km may be experienced in a severe service environment.

If the described condition is experienced, use the front brake pads supplied in kit, P/N 94449206, which is available from GM Parts for replacement use.

If the front pads are replaced due to the early wear condition, the rotors should be inspected for roughness and resurfaced if required or replaced,if wear exceeds serviceability guidelines.

Use applicable labour time and operation number.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.