SMU - SECTION 1B-R-134A POLYALKYENE GLYCOL (PAG). Geo Sprint 1994

For 1990-2009 cars

# SMU - SECTION 1B-R-134A POLYALKYENE GLYCOL (PAG)

********************************************************************** SERVICE MANUAL UPDATE **********************************************************************

#### SUBJECT: SECTION 1B - R134A POLYALKYLENE GLYCOL (PAG) REFRIGERANT OIL

#### MODELS: 1994 GEO METRO, PRIZM AND TRACKER

ALL 1994 GEO VEHICLES MUST USE POLYALKYLENE GLYCOL (PAG) REFRIGERANT OIL, GM P/N 12345923.

#### PART AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.