SERVICE MANUAL UPDATE BRAKE BOOSTER ADJUST.. Geo Tracker - 4WD 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE BRAKE BOOSTER ADJUST.

********************************************************************** SERVICE MANUAL UPDATE GEO METRO SERVICE MANUALS PAGE 5-49 GEO TRACKER SERVICE MANUALS PAGE 5D-1 **********************************************************************

IN THE BRAKE BOOSTER ADJUSTMENT PROCEDURE FOUND ON PAGE 5-49 OF THE 1989-91 GEO METRO SERVICE MANUALS (ST370-89, ST370-90 AND ST370-91, RESPECTIVELY) AND ON PAGE 5D-1 (FIGURES 2 AND 3) OF THE 1989-91 GEO TRACKER SERVICE MANUALS (ST377-89, ST377-90 AND ST377-91, RESPECTIVELY, THERE IS A DISCREPANCY IN THE KENT-MOORE TOOL NUMBER FOR THE BOOSTER PISTON ROD GAGE. THE J-39567 BOOSTER PISTON ROD GAGE SHOULD BE USED, NOT J-34873-A (FIGURES 1 AND 2).

INSERT ART: NC5518-5D2-M-RS FIGURE 1 BRAKE BOOSTER ADJUSTMENT (1 OF 2)

INSERT ART: NC5519-5D2-M-RS FIGURE 1 BRAKE BOOSTER ADJUSTMENT (2 OF 2)

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1992 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.